# waubonsie-subwatershed

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: Mustafa Rahim, Illinois State Water Survey
      Publication_Date: February 2007
      Title:
        waubonsie-subwatershed
      Geospatial_Data_Presentation_Form: vector digital data
      Other_Citation_Details:
        Singh J.et al. 2007. Fox River Watershed Investigation: Stratton Dam to the Illinois River PHASE II, Hydrologic and Water Quality Simulation Models, Part 1: Methodology and Procedures for Development of HSPF Models, Illinois State Water Survey, Champaign, IL.
  Description:
    Abstract:

        This sub watershed file is created for Waubonsie Creek through BASINS automatic delineation tool. BASINS generated outlet shape file waubonsie-outlet-final.shp has been used for sub watershed delineation. During the watershed delineation process, 200 ha of threshold area have been applied for stream definition. NED 1/3 arc second (~ 10 meter resolution) DEM in integer, Z unit in centimeter; downloaded from USGS Seamless data distribution center is also used for watershed delineation.The NED data was downloaded in March 2005. This delineation is completed after resolving the boundary discrepancy and without any modification in DEM.

    Purpose:

        HSPF (Hydrological Simulation Program--Fortran) modeling for the project: Fox River Watershed Investigation, Stratton Dam to the Illinois River - Phase II

  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: February 2007
    Currentness_Reference:

        publication date

  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: As needed
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -88.356515
      East_Bounding_Coordinate: -88.186181
      North_Bounding_Coordinate: 41.791155
      South_Bounding_Coordinate: 41.661219
  Keywords:
    Theme:
      Theme_Keyword: Subwatershed Boundary, Waubonsie Creek
  Access_Constraints: none
  Use_Constraints:

      none

  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Sally McConkey
        Contact_Organization: Illinois State Water Survey
      Contact_Address:
        Address_Type: mailing and physical address
        Address:

            2204 Griffith Dr.

        City: Champaign
        State_or_Province: Illinois
        Postal_Code: 61820-7495
      Contact_Voice_Telephone: (217) 333-5482
      Contact_Electronic_Mail_Address: sally@uiuc.edu
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.1.0.722

Back to Top

Data_Quality_Information:
  Lineage:
    Process_Step:
      Process_Description:

          ESRI ArcGIS to process input GIS layers,
          BASINS 3.1 - Automatic Delineation Tool for watershed and subwatershed delineation,
          ArcCatalog to complete metadata

      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Mustafa Rahim
            Contact_Organization: Illinois State Water Survey
          Contact_Electronic_Mail_Address: rahim@uiuc.edu
    Process_Step:
      Process_Description:

          Metadata imported.

      Source_Used_Citation_Abbreviation:
        C:\FOX-WEB\metadata-subwatershed-nonmod.xml

Back to Top

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: G-polygon
      Point_and_Vector_Object_Count: 7

Back to Top

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: Universal Transverse Mercator
        Universal_Transverse_Mercator:
          UTM_Zone_Number: 16
          Transverse_Mercator:
            Scale_Factor_at_Central_Meridian: 0.999600
            Longitude_of_Central_Meridian: -87.000000
            Latitude_of_Projection_Origin: 0.000000
            False_Easting: 500000.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.000032
          Ordinate_Resolution: 0.000032
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Back to Top

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: waubonsie-subwatershed
    Attribute:
      Attribute_Label: FID
      Attribute_Definition:

          Internal feature number.

      Attribute_Definition_Source:

          ESRI

      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition:

          Feature geometry.

      Attribute_Definition_Source:

          ESRI

      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Coordinates defining the features.
    Attribute:
      Attribute_Label: ID
    Attribute:
      Attribute_Label: GRIDCODE
    Attribute:
      Attribute_Label: SUBBASIN
    Attribute:
      Attribute_Label: AREA
    Attribute:
      Attribute_Label: LEN1
    Attribute:
      Attribute_Label: SLO1
    Attribute:
      Attribute_Label: SLL
    Attribute:
      Attribute_Label: CSL
    Attribute:
      Attribute_Label: WID1
    Attribute:
      Attribute_Label: DEP1
    Attribute:
      Attribute_Label: LATITUDE
    Attribute:
      Attribute_Label: ELEV
    Attribute:
      Attribute_Label: BNAME

Back to Top

Distribution_Information:
  Resource_Description: Downloadable Data
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 0.166
  Technical_Prerequisites:
    ESRI ArcGIS, ArcView 3x software

Back to Top

Metadata_Reference_Information:
  Metadata_Date: 20070413
  Metadata_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Mustafa Rahim
        Contact_Organization: Illinois State Water Survey
      Contact_Address:
        Address_Type: mailing and physical address
        Address:

            2204 Griffith Dr.

        City: Champaign
        State_or_Province: Illinois
        Postal_Code: 61820-7495
      Contact_Voice_Telephone: (217) 265 6713
      Contact_Electronic_Mail_Address: rahim@uiuc.edu
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: http://www.esri.com/metadata/esriprof80.html
    Profile_Name: ESRI Metadata Profile

Back to Top