# tyler-subwatershed

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: Mustafa Rahim, Illinois State Water Survey
      Publication_Date: February 2007
      Title:
        tyler-subwatershed
      Geospatial_Data_Presentation_Form: vector digital data
      Other_Citation_Details:
        Singh J.et al. 2007. Fox River Watershed Investigation: Stratton Dam to the Illinois River PHASE II, Hydrologic and Water Quality Simulation Models, Part 1: Methodology and Procedures for Development of HSPF Models, Illinois State Water Survey, Champaign, IL.
  Description:
    Abstract:

        This sub watershed file is created for Tyler Creek through BASINS automatic delineation tool. BASINS generated outlet shape file tyler-outlet-final.shp has been used for sub watershed delineation. During the watershed delineation process, 200 ha of threshold area have been applied for stream definition. NED 1/3 arc second (~ 10 meter resolution) DEM in integer, Z unit in centimeter; downloaded from USGS Seamless data distribution center is also used for watershed delineation.The NED data was downloaded in March 2005. This delineation is processed with a modified DEM after resolving the boundary discrepancy.

    Purpose:

        HSPF (Hydrological Simulation Program--Fortran) modeling for the project: Fox River Watershed Investigation, Stratton Dam to the Illinois River - Phase II

  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: February 2007
    Currentness_Reference:

        publication date

  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: As needed
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -88.491620
      East_Bounding_Coordinate: -88.287009
      North_Bounding_Coordinate: 42.127046
      South_Bounding_Coordinate: 42.016933
  Keywords:
    Theme:
      Theme_Keyword: Subwatershed Boundary, Tyler Creek
  Access_Constraints: none
  Use_Constraints:

      none

  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Sally McConkey
        Contact_Organization: Illinois State Water Survey
      Contact_Address:
        Address_Type: mailing and physical address
        Address:

            2204 Griffith Dr.

        City: Champaign
        State_or_Province: Illinois
        Postal_Code: 61820-7495
      Contact_Voice_Telephone: (217) 333-5482
      Contact_Electronic_Mail_Address: sally@uiuc.edu
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.1.0.722

Back to Top

Data_Quality_Information:
  Lineage:
    Process_Step:
      Process_Description:

          ESRI ArcGIS to process input GIS layers,
          BASINS 3.1 - Automatic Delineation Tool for watershed and subwatershed delineation,
          ArcCatalog to complete metadata

      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: Mustafa Rahim
            Contact_Organization: Illinois State Water Survey
          Contact_Electronic_Mail_Address: rahim@uiuc.edu
    Process_Step:
      Process_Description:

          Metadata imported.

      Source_Used_Citation_Abbreviation:
        C:\FOX-WEB\metadata-subwatershed-mod.xml

Back to Top

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: G-polygon
      Point_and_Vector_Object_Count: 20

Back to Top

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: Universal Transverse Mercator
        Universal_Transverse_Mercator:
          UTM_Zone_Number: 16
          Transverse_Mercator:
            Scale_Factor_at_Central_Meridian: 0.999600
            Longitude_of_Central_Meridian: -87.000000
            Latitude_of_Projection_Origin: 0.000000
            False_Easting: 500000.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.000032
          Ordinate_Resolution: 0.000032
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Back to Top

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: tyler-subwatershed
    Attribute:
      Attribute_Label: FID
      Attribute_Definition:

          Internal feature number.

      Attribute_Definition_Source:

          ESRI

      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition:

          Feature geometry.

      Attribute_Definition_Source:

          ESRI

      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Coordinates defining the features.
    Attribute:
      Attribute_Label: ID
    Attribute:
      Attribute_Label: GRIDCODE
    Attribute:
      Attribute_Label: SUBBASIN
    Attribute:
      Attribute_Label: AREA
    Attribute:
      Attribute_Label: LEN1
    Attribute:
      Attribute_Label: SLO1
    Attribute:
      Attribute_Label: SLL
    Attribute:
      Attribute_Label: CSL
    Attribute:
      Attribute_Label: WID1
    Attribute:
      Attribute_Label: DEP1
    Attribute:
      Attribute_Label: LATITUDE
    Attribute:
      Attribute_Label: ELEV
    Attribute:
      Attribute_Label: BNAME

Back to Top

Distribution_Information:
  Resource_Description: Downloadable Data
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 0.287
  Technical_Prerequisites:
    ESRI ArcGIS, ArcView 3x software

Back to Top

Metadata_Reference_Information:
  Metadata_Date: 20070413
  Metadata_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Mustafa Rahim
        Contact_Organization: Illinois State Water Survey
      Contact_Address:
        Address_Type: mailing and physical address
        Address:

            2204 Griffith Dr.

        City: Champaign
        State_or_Province: Illinois
        Postal_Code: 61820-7495
      Contact_Voice_Telephone: (217) 265 6713
      Contact_Electronic_Mail_Address: rahim@uiuc.edu
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: http://www.esri.com/metadata/esriprof80.html
    Profile_Name: ESRI Metadata Profile

Back to Top